**Encouraging the operators to use the welding hood correctly**

*We want to ensure that the hood is positioned within the distance as determined by the smoke assessment for maximum capture.*

*Show the operator the smoke assessment and label the hood with the results:*

**THIS HOOD MUST BE PLACED NO MORE THAN**

 **mm**

**FROM THE SOURCE OF EMMISSIONS**

**;**

**HOOD

SOURCE OF EMMISSIONS

**MAXIMUM**

**DISTANCE*****Perhaps label the hood with a diagram of what the capture distance means:*

*.*

© Airducts Design Ltd